From fe86c7399d9bc20f7f95f7557d6d2b80e7b86be3 Mon Sep 17 00:00:00 2001
From: Adrian Kummerlaender
Date: Tue, 29 Jan 2019 15:23:53 +0100
Subject: Revamp gnuplot plotting to generate better output

Using the pdfcairo terminal for generating fluid flow plots in gnuplot
using raw paraview-generated CSV exports generates high quality results.
Sadly the resulting files are both unoptimized and quite big which leads
to both large and unperformant documents (i.e. some PDF readers even crash)

As an alternative this new gnuplot structure generates the fluid plot
itself using the pngcairo terminal and includes the resulting
high-resolution PNG image into a normal pdfcairo plot. This works out
quite well.

As a side benefit the plot scripts are now much easier to maintain.
---
 content.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 241be7e..80127dd 100644
--- a/content.tex
+++ b/content.tex
@@ -938,7 +938,7 @@ Für die Umsetzung in OpenLB parametrisieren wir die Geometrie bezogen auf den Z
 
 \begin{figure}[h]
 \begin{adjustbox}{center}
-\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_unrefined_60s_full.pdf}
+\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_unrefined_60s.pdf}
 \end{adjustbox}
 \caption{Uniform mit \(N=20\) aufgelöstes Strömungsbild zu \(t=60s\)}
 \label{fig:UniformCylinderVelocity60s}
@@ -948,7 +948,7 @@ Als Grundlage für den subjektiven Vergleich des Strömungsbildes simulieren wir
 
 \begin{figure}[h]
 \begin{adjustbox}{center}
-\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_single_refinement_60s_full.pdf}
+\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_single_refinement_60s.pdf}
 \end{adjustbox}
 \caption{Einfach verfeinertes Strömungsbild zu \(t=60s\)}
 \label{fig:SingleLevelRefinementCylinderVelocity60s}
@@ -963,7 +963,7 @@ An dieser Stelle wollen wir die Gelegenheit nutzen, uns näher mit der Wahl der
 
 \begin{figure}[h]
 \begin{adjustbox}{center}
-\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_unrefined_60s_knudsen_full.pdf}
+\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_unrefined_60s_knudsen.pdf}
 \end{adjustbox}
 \caption{Verfeinerungskriterium in einem uniform aufgelösten Gitter zu \(t=60s\)}
 \label{fig:UnrefinedCylinderKnudsen60s}
@@ -974,7 +974,7 @@ Große Teile des Gitters weisen demnach eine gute Auflösung mit Verfeinerungsfa
 
 \begin{figure}[h]
 \begin{adjustbox}{center}
-\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_single_refinement_60s_knudsen_full.pdf}
+\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_single_refinement_60s_knudsen.pdf}
 \end{adjustbox}
 \caption{Verfeinerungskriterium in einem einfach verfeinerten Gitter zu \(t=60s\)}
 \label{fig:SingleLevelRefinementCylinderKnudsen60s}
@@ -984,7 +984,7 @@ Insgesamt war unter dieser formaleren Analyse unsere intuitive Wahl des in Abbil
 
 \begin{figure}[h]
 \begin{adjustbox}{center}
-\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_improved_grid_60s_knudsen_full.pdf}
+\includegraphics[width=1.2\textwidth]{img/static/cylinder2d_improved_grid_60s_knudsen.pdf}
 \end{adjustbox}
 \end{figure}
 
-- 
cgit v1.2.3

